
This folder contains the new proprietary 10Micron ASCOM driver version 1.0 
that can be useful in integrating the 10micron mounts with third party 
controlling softwares.


This folder contains also ASCOM free third-party drivers that can be useful in
integrating the 10micron mounts with controlling softwar:


The Meade LX200 Classic driver (MeadeClassic(5.0.3)Setup.exe) is built by
a collaboration of various authors: Robert B. Denny, Chris Rowland,
Chris Creery, Larry Weber, Jon Brewster, Jonathan Putsman. Portions
copyright © 2001, SPACE.com Canada, Ltd. and copyright © 2002, Diffraction
Limited. The Meade LX200 Classic driver is distributed under the Creative
Commons Attribution-NoDerivs 3.0 Unported license. You can find the full
license at this link:

http://creativecommons.org/licenses/by-nd/3.0/



All these drivers require the ASCOM platform version 5 or above to be 
installed. Install the ASCOM platform from the included file, or 
(better) download the last version from the website
http://ascom-standards.org/



DISCLAIMER:

10Micron makes no warranties regarding these softwares, express or implied,
as to its suitability or fitness for a particular purpose.
