Clock Sync software, version 3.4 - Copyright COMEC S.n.c. 2015

10Micron Clock Sync3.4

--- Usage ---

In the "Mount address" box, insert the IP address of the mount (for example 192.168.1.99) or the COM port it is 
connected to (for example COM1).

Select "Keep mount synchronized" in the "Sync mode" selector.

Click on connect. The program will connect to the mount and send periodically a command to adjust the clock.

Usually you will keep selected "Do not sync while tracking", since sometimes setting the clock may cause a small "jump" 
while the mount is tracking. The clock will be updated when the mount is slewing to a target, or when the mount is stopped 
or parked.

If "Auto connect" is checked, the program will try to connect to the mount continuously, even if the mount is not found. 
This setting is retained at the next startup.

